Wearables computing exercise code book

I do not know very well what to write here.

I have imported and respected all variables names used by the reasearchers. I have just cleaned them a little, to remove dashes. The meaning of the variables and the units in which they are expressed are the ones explained in the original research code book, or readme file.

Example:

|  |  |  |  |
| --- | --- | --- | --- |
| tBodyAccmean()X | tBodyAccmean()Y | tBodyAccmean()Z | tBodyAccstd()X… |

There are in total 66 extracted variables, whose means are calculated in the second part of the exercise.

Plus, the variables for subjects and activities:

subject: numbers 1 to 30 for the individuals that were subjects in the study.

activity: id number for each of the six activity types

activityname: name of the activity, i.e.:

|  |
| --- |
| activityname |
| LAYING |
| SITTING |
| STANDING |
| WALKING |
| WALKING\_DOWNSTAIRS |
| WALKING\_UPSTAIRS |

For reference, I have copied below the content of the original README file for the research.

==================================================================

Human Activity Recognition Using Smartphones Dataset

Version 1.0

==================================================================

Jorge L. Reyes-Ortiz, Davide Anguita, Alessandro Ghio, Luca Oneto.

Smartlab - Non Linear Complex Systems Laboratory

DITEN - Università degli Studi di Genova.

Via Opera Pia 11A, I-16145, Genoa, Italy.

activityrecognition@smartlab.ws

www.smartlab.ws

==================================================================

The experiments have been carried out with a group of 30 volunteers within an age bracket of 19-48 years. Each person performed six activities (WALKING, WALKING\_UPSTAIRS, WALKING\_DOWNSTAIRS, SITTING, STANDING, LAYING) wearing a smartphone (Samsung Galaxy S II) on the waist. Using its embedded accelerometer and gyroscope, we captured 3-axial linear acceleration and 3-axial angular velocity at a constant rate of 50Hz. The experiments have been video-recorded to label the data manually. The obtained dataset has been randomly partitioned into two sets, where 70% of the volunteers was selected for generating the training data and 30% the test data.

The sensor signals (accelerometer and gyroscope) were pre-processed by applying noise filters and then sampled in fixed-width sliding windows of 2.56 sec and 50% overlap (128 readings/window). The sensor acceleration signal, which has gravitational and body motion components, was separated using a Butterworth low-pass filter into body acceleration and gravity. The gravitational force is assumed to have only low frequency components, therefore a filter with 0.3 Hz cutoff frequency was used. From each window, a vector of features was obtained by calculating variables from the time and frequency domain. See 'features\_info.txt' for more details.

For each record it is provided:

======================================

- Triaxial acceleration from the accelerometer (total acceleration) and the estimated body acceleration.

- Triaxial Angular velocity from the gyroscope.

- A 561-feature vector with time and frequency domain variables.

- Its activity label.

- An identifier of the subject who carried out the experiment.

The dataset includes the following files:

=========================================

- 'README.txt'

- 'features\_info.txt': Shows information about the variables used on the feature vector.

- 'features.txt': List of all features.

- 'activity\_labels.txt': Links the class labels with their activity name.

- 'train/X\_train.txt': Training set.

- 'train/y\_train.txt': Training labels.

- 'test/X\_test.txt': Test set.

- 'test/y\_test.txt': Test labels.

The following files are available for the train and test data. Their descriptions are equivalent.

- 'train/subject\_train.txt': Each row identifies the subject who performed the activity for each window sample. Its range is from 1 to 30.

- 'train/Inertial Signals/total\_acc\_x\_train.txt': The acceleration signal from the smartphone accelerometer X axis in standard gravity units 'g'. Every row shows a 128 element vector. The same description applies for the 'total\_acc\_x\_train.txt' and 'total\_acc\_z\_train.txt' files for the Y and Z axis.

- 'train/Inertial Signals/body\_acc\_x\_train.txt': The body acceleration signal obtained by subtracting the gravity from the total acceleration.

- 'train/Inertial Signals/body\_gyro\_x\_train.txt': The angular velocity vector measured by the gyroscope for each window sample. The units are radians/second.

Notes:

======

- Features are normalized and bounded within [-1,1].

- Each feature vector is a row on the text file.

For more information about this dataset contact: activityrecognition@smartlab.ws

License:

========

Use of this dataset in publications must be acknowledged by referencing the following publication [1]

[1] Davide Anguita, Alessandro Ghio, Luca Oneto, Xavier Parra and Jorge L. Reyes-Ortiz. Human Activity Recognition on Smartphones using a Multiclass Hardware-Friendly Support Vector Machine. International Workshop of Ambient Assisted Living (IWAAL 2012). Vitoria-Gasteiz, Spain. Dec 2012

This dataset is distributed AS-IS and no responsibility implied or explicit can be addressed to the authors or their institutions for its use or misuse. Any commercial use is prohibited.

Jorge L. Reyes-Ortiz, Alessandro Ghio, Luca Oneto, Davide Anguita. November 2012.